Two plates, two holes each, and the mount sitting right on top. 
It works exactly as intended and yes, I’m just throwing that in there for the pun. 
I couldn’t find any 5.25" Part for this, so I decided to bridge the gap with this simple part.